**RIP protocol configuration**

Aim :- Configuring RIP Routing Protocol in Routers.

Observation:-

* We used to add routes to routers statically and this may become cumbersome quickly.
* To solve this problem a protocol called RIP protocol was introduced. It copies the routing table of its neighbouring routes. Limit of its extension is 16 nodes in the network.

Outcome:-

* Learnt how to configure RIP protocol.